Copyright 2022 ADVANCED MICRO DEVICES, INC. All Rights Reserved. 

AMD RAID controller driver distribution list
Revision: 9.3.2.00158
Build date: 09/01/2022
OS: Windows10 x64, Windows11 21H2 x64, Windows11 22H2 x64
Driver package:
WIN10\x64\ NVMe_DID (AMD Non-Volatile Memory Express Device ID files)
Supported AMD processors:
•	AMD Ryzen™ Processors
•	AMD Ryzen™ Processors with Radeon™ Graphics.

WIN10\x64\RAID_SATA
•	Supports all raid enabled AMD Ryzen™ Processors (SATA only)

Note:
•	RAID5 is only supported on 3rd and 4th Gen AMD Ryzen™ Threadripper™ Processors

AMD-RAID binary file name:
•	rcraid.cat, rcraid.inf, rcraid.sys
•	rccfg.cat, rccfg.inf, rccfg.sys
•	rcbottom.cat, rcbottom.inf, rcbottom.sys

Known issues
•	Under RaidXpert2 and rcadm.exe, device id for some NVMe shows up as xb000 rather than actual NVMe device ID.
•	No support for 2 ODDs on the same port of 2 different controllers.
•	OS Installation may fail when OS installed on other than first RAID array.
•	Bugcheck 9f during long S3/S4 ACPI Cycles
•	Bugcheck D1 during long S4 ACPI Cycles
•	Hibernate Suspend and resume performance drop in RAID-5 on specific HDD.
•	IO performance impact on VBS enabled systems. 

Revision History
9.3.2.00158
·	RAID IO Performance improvement on Windows 11 22H2.
·	Fix for OS installation on specific NVMe vendor.

9.3.2.00142
·	Bugcheck 9F Issue fix for AM5.
·	Fix for device drop on AM5
·	LED Blink Pattern statement on RAIDXper2 Application.

9.3.2.00130
·	AM5 SATA OS installation issue fix
·	Fix for System Hang during idle period

9.3.2.00121
·	S3/S4 stability related enhancements.

9.3.2.00118
·	Extended feature to support BypassIO
·	Fix timing issue with S4 to address disk offline in Core.
·	Fix for Logs are getting appended, instead of deleting and showing the SMART Values for user requested Device.
·	Help Commands set for "" SMART GET "" do not fetch the desired Information. Enhance current rcadm to display SMART values the RAID driver can currently query instead of reporting ""SMART status not supported on SAS drive X"""
·	Add NVMe Pass Through support to Windows
·	RAID led support and related fixes

9.3.2.00099
·	Enabled Support for increase in number of RAID Array, Storage Controller & Storage Devices.
·	Enabled Support for BypassIO
·	Fix Controller number to match the ctrl:channel info of the disks
·	Add NVMe PassThrough support to Windows
·	Enable RAID LED Blink support